ABOUT THIS APP

MilluminSync

I created this app with Max MSP.
It sends and receives OSC messages using the commands found in the documentation here.
https://github.com/anome/millumin-dev-kit/wiki/OSC-documentation#managing-media

Sending is on port 5000
Receiving is on port 8000

In order for the app to receive messages please enable “API feedback” under the OSC tab of the “Device Manager” (command K).
This will allow the countdown clock, file name, and TRT display to work. (You should only need to do this on your primary machine.)

USAGE

All machines must be on the same network and routable to each other.

Launch the app on your primary machine.

Click Set External IPs button to enter a list of IP addresses, one IP per line, maximum of five IPs. Do not enter the IP address of your primary machine (the machine MilluminSync is running on) MilluminSync finds the local machine automatically. 

Close the text window for entering IP addresses without saving.

Click the Save IPs button.

A file named mlSyncIPsave is created in the same directory as the MilluminSync app. This is where your IP addresses are stored.

CHANGELOG

v1.1 
Added ability to control up to 5 machines.

Have a great show!

JP Kelly
jp@jpkvideo.com

