ABOUT THIS APP

I created this app with Max MSP.
It sends and receives OSC messages using the commands found in the documentation here.
https://github.com/anome/millumin-dev-kit/wiki/OSC-documentation#managing-media

Sending is on port 5000
Receiving is on port 8000

In order for the app to receive messages please enable “API feedback” under the OSC tab of the “Device Manager” (command K).
This will allow the countdown clock, file name, and TRT display to work.

USAGE

Both machines must be on the same network and routable to each other.

Launch the app on your primary machine.

Set “Host 1 IP” to 127.0.0.1 or the routable IP address of your machine.

Set “Host 2 IP” the the IP address of your backup machine.

Have a great show!

JP Kelly
jp@jpkvideo.com

